|  |  |  |  |
| --- | --- | --- | --- |
| **5**  | **Detector Pipe** | Must clear detectors/frames by 3 mmMust clear inner edges of Charged Particle Envelopes by 3 mm including out of roundness and positional toleranceMust clear OPE by 3 mm including all out of roundness and positional tolerance  |   |