|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Traveler Title | C75 HOM Load Brazed Assembly | | | |
| Traveler Abstract | The purpose of this document is to capture the brazing process and run parameters associated with brazing the HOM Load to the Copper Support Pedestal and SS Mounting Flange Assembly. | | | |
| Traveler ID | C75-HOM-BRAZ-ASSY | | | |
| Traveler Revision | R1 | | | |
| Traveler Author | Scott Williams | | | |
| Traveler Date | 5-May-20 | | | |
| NCR Informative Emails | S. Williams, J. Guo, K. Macha, K. Davis, D. Forehand | | | |
| NCR Dispositioners | S. Williams, J. Guo, K. Macha, K. Davis, D. Forehand | | | |
| D3 Emails | S. Williams, J. Guo, K. Macha, K. Davis, D. Forehand | | | |
| Approval Names | S. Williams, , | J. Guo | K. Macha |  |
| Approval Signatures |  |  |  |  |
| Approval Dates |  |  |  |  |
| Approval Title | Author | Reviewer | Project Manager |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| References | List and Hyperlink all documents related to this traveler. This includes, but is not limited to: safety (THAs, SOPs, etc), drawings, procedures, and facility related documents. | | | |
| [C75 HOM Load Assy. JL0024622](../HOM%20Load%20Drawings/JL0024622_B_C75%20HOM%20LOAD.pdf) | [C75 HOM ABSORBER FLANGE JL0024623](../HOM%20Load%20Drawings/JL0024623-B-HOM%20ABSORBER%20FLANGE.pdf) | [C75 HOM LOAD JL0006805](../HOM%20Load%20Drawings/JL0006805_-_C50%20HOM%20LOAD%204.0.pdf) | [C75 HOM PEG BOARD JL0041239](../HOM%20Load%20Drawings/JL0041239_-_C50%20HOM%20PEG%20BOARD(7).pdf) | [C75 HOM Load Retainer JL0027665](../HOM%20Load%20Drawings/JL0027665_A_%20RETAINER%204.0(2).pdf) |
| [C75 HOM Retainer Screw JL0038398](../HOM%20Load%20Drawings/JL0038398_-_SH%20SH%20SCREW%20.125%20D%20X%200.313%20LG%20X%204-40%20THREAD(1).pdf) | [CP-STP-CAV-CHEM-ACID-R1](https://jlabdoc.jlab.org/docushare/dsweb/Get/Document-141848/CP-STP-CAV-CHEM-ACID-R1.pdf) | [CP-STP-CAV-CHEM-DEGR-R3](https://jlabdoc.jlab.org/docushare/dsweb/Get/Document-132364/CP-STP-CAV-CHEM-DEGR-R3.pdf) |  |  |

|  |  |
| --- | --- |
| Revision Note |  |
| R1 | Initial release of this Traveler. |

|  |  |  |
| --- | --- | --- |
| Step No. | Instructions | Data Input |
| 1 | Record Load, Flange, and Copper Pedastal numbers. | [[Technician]] <<USERNAME>>  [[LoadMaterialPO]] <<SN>>  [[SSFlangeSN]] <<SN>>  [[PedastalPO]] <<SN>>  [[Date\_DataCapture]] <<TIMESTAMP>>  [[Comment\_DataCapture]] <<COMMENT>> |
| 2 | Verify that all components are clean and properly packaged prior to use  (HOM Loads, SS Flanges, Cu Pedastals, Fixturing, Braze Alloy, etc.). | [[PartsCleaned]] <<YESNO>>  [[Date\_CleaningStatus]] <<TIMESTAMP>>  [[Comment\_CleaningStatus]] <<COMMENT>> |
| 3 | Handle with gloves & visually inspect ceramic load, SS flange and copper pedastal for imperfections (chipped ceramics, burrs, scratches, staining, oxidation, etc.) | [[Technician\_VisualInspection]] {{Williams,other}} <<SELECT>>  [[Date\_VisualInspection]] <<TIMESTAMP>>  [[Comment\_VisualInspection]] <<COMMENT>> |
| 4 | Using the required ceramic fixturing and molybdenum alignment pins, assemble HOM Load Assembly for brazing. Place .008” Thick Cusil ABA Foil between surfaces to be brazed (SS Flange/Copper Pedestal & Copper Pedestal/HOM Load). | [[Technician\_Assembly]]  {{Williams,other}} <<SELECT>>  [[Date\_Assembly]] <<TIMESTAMP>>  [[Comment\_Assembly]] <<COMMENT>> |
| 5 | Place (2) additional ceramics (approx.. 190 gms Ea.) on top of the ceramic alignment fixture, parallel with (1EA) on each side of load. | [[Technician]] <<USERNAME>>  [[Date]] <<TIMESTAMP>> |
| 6 | Place fixtured brazement on individual 4” alumina wafer, load in furnace with close proximity to thermal couples, initiate braze run, and start Labview temperature profile recording. | [[Technician\_BrazeRun]] {{Williams,other}} <<SELECT>>  [[Date\_BrazeRun]] <<TIMESTAMP>>  [[Comment\_BrazeRun]] <<COMMENT>> |
|  |  |  |
| 7 | Record brazing program run profile number and upload Labview Temperature Profile file of braze run. | [[Technician\_ProfileDataNo1]] {{Williams,other}} <<SELECT>>  [[BrazementSN]] <<SN>>  [[FurnaceUsedNo1]] {{Big Blue,Little Blue}} <<SELECT>>  [[ProgramName\_LittleBlueNo1]] <<FLOAT>>  [[ProgramProfileNo\_BigBlueNo1]] {{1,2,3,4,5,6,7,8,9,10}} <<SELECT>>  [[TemperatureProfileFileNo1]] <<FILEUPLOAD>>  [[QuantityOfPartsRanNo1]] <<INTEGER>>  [[Date\_ProfileDataNo1]] <<TIMESTAMP>>  [[Comment\_ProfileDataNo1]] <<COMMENT>> |
| 8 | Vent furnace once cooled, remove brazed HOM Load Assembly, and visually inspect ( alignment retained, proper alloy wetting, good adhesion, chipping of load material, discolorations, etc…). | [[Technician]] <<USERNAME>>  [[Date\_VisualInspection ]] <<TIMESTAMP>>  [[VisualInspection]] <<COMMENT>> |
| 9 | Install Load Retainer onto brazement as per drawing [C75 HOM Load Assy. JL0024622](file:///\\jlabhome\home\scott\Jde\Scotts%20Work%20J\SRF%20Work\HOM%20Load%20Drawings\JL0024622_B_C75%20HOM%20LOAD.pdf), torqueing shoulder screws to 4 in/lbs as noted on drawing. | [[Technician]] <<USERNAME>>  [[Date\_RetainerInstall ]] <<TIMESTAMP>>  [[RetainerInstall]] <<COMMENT>> |
| 10 | Verify HOM Load Assembly is complete and ready to proceed to QA Work Center for final inspection. | [[Technician]] <<USERNAME>>  [[Date\_AssemblyCompletion ]] <<TIMESTAMP>>  [[AssemblyCompletion]] <<COMMENT>> |