|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Traveler Title | H-HOM Feedthrough 25ohm Pince | | | |
| Traveler Abstract | Outlines the inspection of the HOM Feedthrough 25ohm Pince | | | |
| Traveler ID | AUP-INSP-CMN-FTPCSN | | | |
| Traveler Revision | R1 | | | |
| Traveler Author | Matthew Weaks | | | |
| Traveler Date | 30-Mar-20 | | | |
| NCR Informative Emails | weaksmc | | | |
| NCR Dispositioners | Huque | | | |
| D3 Emails | Huque | | | |
| Approval Names | Matthew Weaks | Scott Williams | Naeem Huque |  |
| Approval Signatures |  |  |  |  |
| Approval Dates |  |  |  |  |
| Approval Title | Author | Reviewer | Project Manager |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| References | List and Hyperlink all documents related to this traveler. This includes, but is not limited to: safety (THAs, SOPs, etc), drawings, procedures, and facility related documents. | | | |
| [CP-AUP-CAV-CHEM-DEGR](https://jlabdoc.jlab.org/docushare/dsweb/Get/Document-212638/CP-AUP-CAV-CHEM-DEGR-R1.pdf) | Drawing Link? | ASTM F68 as per CERN No. 2001 Ed. 8 and EDMS No. 790779 link? |  |  |
|  |  |  |  |  |

|  |  |
| --- | --- |
| Revision Note |  |
| R1 | Initial release of this Traveler. |

|  |  |  |
| --- | --- | --- |
| Step No. | Instructions | Data Input |
| 1 | Serial Number of Part | [[FTPCSNSN]] <<SN>> |
| Confirm JL0089757 Material Specification meets ASTM F68 as per CERN No. 2001 Ed. 8 and EDMS No. 790779.  Upload Material Certification, as well as any relevant photos and/or comments. | [[Ins1Tech]] <<USERNAME>>  [[Ins1Time]] <<TIMESTAMP>>  [[Ins1Comm]] <<COMMENT>>  [[Ins1Cert]] <<FILEUPLOAD>> |
| 2 | Machine the component as per drawing JL0089757  Upload any relevant documents and/or photos. | [[MachTech]] <<USERNAME>>  [[MachTime]] <<TIMESTAMP>>  [[MachComm]] <<COMMENT>>  [[MachFile]] <<FILEUPLOAD>> |
| 3 | Degrease JL0089757 as per JLab CP-AUP-CAV-CHEM-DEGR.  Upload any relevant photos and/or comments. | [[DG1Tech]] <<USERNAME>>  [[DG1Time]] <<TIMESTAMP>>  [[DG1Comm]] <<COMMENT>>  [[DG1File]] <<FILEUPLOAD>> |
| 4 | Verify dimensions marked on JL0089757\_CMM.  Upload inspection report. | [[Ins2Tech]] <<USERNAME>>  [[Ins2Time]] <<TIMESTAMP>>  [[Ins2Comm]] <<COMMENT>>  [[Ins2File]] <<FILEUPLOAD>> |