|  |  |
| --- | --- |
| Traveler Title | Cebaf Cryomodule Dogleg Window Assembly |
| Traveler Abstract | This traveler details the steps required to dimensionally inspect the Dogleg window assembly for Cebaf Reworked Cryomodule |
| Traveler ID | C50R-CPR-INSP-DGLG |
| Traveler Revision  | R1 |
| Traveler Author | A. DeKerlegand |
| Traveler Date | 19-Jan-2021 |
| NCR Informative Emails | macha |
| NCR Dispositioners | Forehand,kdavis,scott |
| D3 Emails | Forehand,kdavis,scott,areilly |
| Approval Names | A. DeKerlegand | S.Williams | K. Macha |  |
| Approval Signatures |  |  |  |  |
| Approval Dates |  |  |  |  |
| Approval Title | Author | Reviewer | Project Manager |  |

|  |  |
| --- | --- |
| References | List and Hyperlink all documents related to this traveler. This includes, but is not limited to: safety (THAs, SOPs, etc), drawings, procedures, and facility related documents. |
| [CRM0882025-0002](https://jlabdoc.jlab.org/docushare/dsweb/Get/Document-72037/crm0882025-0002.pdf) | [CRM-088-2025-0002Rev C](https://jlabdoc.jlab.org/docushare/dsweb/Get/Document-234995/CRM0882025-0002%20REV%20C.pdf) |  |  |  |
|  |  |  |  |  |

|  |  |
| --- | --- |
| Revision Note |  |
| R1 | Initial release of this Traveler. |

|  |  |  |
| --- | --- | --- |
| Step No. | Instructions | Data Input |
| 1 | Record Serial number of Dogleg Window/FPC Extension Assembly | [[DGLGSN]] <<DGLGSN>> |
| 2 | Verify the following dimensions. Use table A when window is at the weldment stage. If necessary, bend small flange so that holes 1 and 2 meet the true position tolerance and parallelism as listed below.  | [[Dim1VerifyTech]] <<SRF>> [[Dim1VerifyDate]] <<TIMESTAMP>> [[Dim1Comments]] <<COMMENT>> |
| **Drawing Number** | **Description-Table A** | **Drawing Value** | **Tolerance** | **Measured Value** |
| CRM-088-2025-0002 | True Position of hole 1 | .015 | Max. | [[MeasValue1]] <<FLOAT>> |
| CRM-088-2025-0002 | True Position of hole 2 | .015 | Max. | [[MeasValue2]] <<FLOAT>> |
| CRM-088-2025-0002 | Parallelism of small flange | .010 | Max. | [[MeasValue3]] <<FLOAT>> |
| CRM-088-2025-0002 | Location of hole 1 (X) | .000 |  | [[MeasValue4]] <<FLOAT>> |
| CRM-088-2025-0002 | Location of hole 1 (Y) | .000 |  | [[MeasValue5]] <<FLOAT>> |
| CRM-088-2025-0002 | Location of hole 2 (X) | .000 |  | [[MeasValue6]] <<FLOAT>> |
| CRM-088-2025-0002 | Location of hole 2 (Y) | .000 |  | [[MeasValue7]] <<FLOAT>> |
| CRM-088-2025-0002 | Location of small flange (X) | .000 |  | [[MeasValue8]] <<FLOAT>> |
| CRM-088-2025-0002 | Location of small flange (Y) | .000 |  | [[MeasValue9]] <<FLOAT>> |

|  |  |  |
| --- | --- | --- |
| Step No. | Instructions | Data Input |
| 3 | *Post machining step.* With CMM verify the following dimensions. If necessary, bend small flange so that holes 1 and 2 meet the true position tolerance and parallelism listed below. Note: Eyelet pocket depth tolerance listed below is different from drawing to allow for lapping material removal. | [[Dim2VerifyTech]] <<SRF>> [[Dim2VerifyDate]] <<TIMESTAMP>> [[Dim2Comments]] <<COMMENT>> |
| **Drawing Number** | **Description** | **Drawing Value** | **Tolerance** | **Measured Value** |
| CRM-088-2025-0002 | Height of wave guide assembly | 6.732 | + - .005 | [[MeasValue10]] <<FLOAT>> |
| CRM-088-2025-0002 | Parallelism of small flange | .002 | Max. | [[MeasValue11]] <<FLOAT>> |
| CRM-088-2025-0002 | True Position of hole\_1 | .020 | Max. | [[MeasValue12]] <<FLOAT>> |
| CRM-088-2025-0002 | True Position of hole\_2 | .020 | Max. | [[MeasValue13]] <<FLOAT>> |
| CRM-088-2025-0002 | Pocket Depth | .032 | +.005 / -.005 | [[MeasValue14]] <<FLOAT>> |
| CRM-088-2025-0002 | Iris depth | .377 | + - .010 | [[MeasValue15]] <<FLOAT>> |
| CRM-088-2025-0002 | Location of hole\_1 (X) | .000 |  | [[MeasValue16]] <<FLOAT>> |
| CRM-088-2025-0002 | Location of hole\_1 (Y) | .000 |  | [[MeasValue17]] <<FLOAT>> |
| CRM-088-2025-0002 | Location of hole\_2 (X) | .000 |  | [[MeasValue18]] <<FLOAT>> |
| CRM-088-2025-0002 | Location of hole\_2 (Y) | .000 |  | [[MeasValue19]] <<FLOAT>> |
| CRM-088-2025-0002 | Location of small flange (X) | .000 |  | [[MeasValue20]] <<FLOAT>> |
| CRM-088-2025-0002 | Location of small flange (Y) | .000 |  | [[MeasValue21]] <<FLOAT>> |

|  |  |  |
| --- | --- | --- |
| Step No. | Instructions | Data Input |
| 4 | *FINAL CMM INSPECTION.* Verify the following dimensions. If necessary, bend small flange so that holes 1 and 2 meet the true position tolerance and parallelism listed below.  | [[Dim3VerifyTech]] <<SRF>> [[Dim3VerifyDate]] <<TIMESTAMP>> [[Dim3Comments]] <<COMMENT>> |
| **Drawing Number** | **Description** | **Drawing Value** | **Tol.** | **Measured Value** | **Within Tol.** |
| CRM-088-2025-0002 | Height of wave guide assembly | 6.722 | + - .005 | [[MeasValue22]] <<FLOAT>> | [[Tolerance1]] <<YESNO>> |
| CRM-088-2025-0002 | Large flange flatness | .002 | Max. | [[MeasValue23]] <<FLOAT>> | [[Tolerance2]] <<YESNO>> |
| CRM-088-2025-0002 | Small flange flatness | .002 | Max. | [[MeasValue24]] <<FLOAT>> | [[Tolerance3]] <<YESNO>> |
| CRM-088-2025-0002 | Parallelism of small flange | .002 | Max. | [[MeasValue25]] <<FLOAT>> | [[Tolerance4]] <<YESNO>> |
| CRM-088-2025-0002 | True Position of hole\_1 | .020 | Max. | [[MeasValue26]] <<FLOAT>> | [[Tolerance5]] <<YESNO>> |
| CRM-088-2025-0002 | True Position of hole\_2 | .020 | Max. | [[MeasValue27]] <<FLOAT>> | [[Tolerance6]] <<YESNO>> |
| CRM-088-2025-0002 | True Position of small flange | .020 | Max. | [[MeasValue28]] <<FLOAT>> | [[Tolerance7]] <<YESNO>> |
| CRM-088-2025-0002 | Location of small flange (X) | .000 |  | [[MeasValue29]] <<FLOAT>> | [[Tolerance8]] <<YESNO>> |
| CRM-088-2025-0002 | Location of small flange (Y) | .000 |  | [[MeasValue30]] <<FLOAT>> | [[Tolerance9]] <<YESNO>> |
| CRM-088-2025-0002 | Location of hole\_1 (X) | .000 |  | [[MeasValue31]] <<FLOAT>> | [[Tolerance10]] <<YESNO>> |
| CRM-088-2025-0002 | Location of hole\_1 (Y) | .000 |  | [[MeasValue32]] <<FLOAT>> | [[Tolerance11]] <<YESNO>> |
| CRM-088-2025-0002 | Location of hole\_2 (X) | .000 |  | [[MeasValue33]] <<FLOAT>> | [[Tolerance12]] <<YESNO>> |
| CRM-088-2025-0002 | Location of hole\_2 (Y) | .000 |  | [[MeasValue34]] <<FLOAT>> | [[Tolerance13]] <<YESNO>> |
| CRM-088-2025-0002 | Point on small flange – concave side *REFERENCE ONLY* | .000 |  | [[MeasValue35]] <<FLOAT>> |  |
| CRM-088-2025-0002 | Point on small flange – convex side *REFERENCE ONLY* | .000 |  | [[MeasValue36]] <<FLOAT>> |  |
| CRM-088-2025-0002 | Angle of twist on small flange*REFERENCE ONLY* | n/a |  | [[MeasValue37]] <<FLOAT>> |  |

|  |  |  |
| --- | --- | --- |
| Step No. | Instructions | Data Input |
| 5 | Verify the surface finish of the large and small flanges using the Mitutoyo Profilometer. | [[Dim4VerifyTech]] <<SRF>> [[Dim4VerifyDate]] <<TIMESTAMP>> [[Dim4Comments]] <<COMMENT>> |
| **Drawing Number** | **Description** | **Has Flange had BCP ?**  | **Drawing Value** | **Measured Value** | **Within Tolerance** |
| CRM-088-2025-0002 | Large flange surface finish | [[FlangeBCP1]] <<YESNO>> | 32 | [[MeasValue38]] <<FLOAT>> | [[Tolerance14]] <<YESNO>> |
| CRM-088-2025-0002 | Small flange surface finish | [[FlangeBCP2]] <<YESNO>> | 32 | [[MeasValue39]] <<FLOAT>> | [[Tolerance15]] <<YESNO>> |

|  |  |  |
| --- | --- | --- |
| Step No. | Instructions | Data Input |
| 6 | Final Visual. Verify flanges are free of damage, pits and scratches. | [[Dim5VerifyTech]] <<SRF>> [[Dim5VerifyDate]] <<TIMESTAMP>> [[Dim5Comments]] <<COMMENT>> |
| **Drawing Number** | **Description** | **Flange Visual** |  |  |  |
| CRM-088-2025-0002 | Large flange  | Large flange okay? | [[Flange40]] <<YESNO>> |  |  |
| CRM-088-2025-0002 | Small flange | Small flange okay? | [[Flange41]] <<YESNO>> |  |  |