|  |  |
| --- | --- |
| Traveler Title | LCLS-II HE 2K Clamp Assembly Kit Inspection Traveler |
| Traveler Abstract | This traveler covers the necessary steps to perform incoming inspection and acceptance of LCLS-II HE 2K clamp assembly kit at JLab. This item is a Fermilab procurement and drop-shipped to JLab. |
| Traveler ID | L2HE INSP-CLMP02K |
| Traveler Revision  | R1 |
| Traveler Author | Seetha-Lakshmi Lalitha |
| Traveler Date | 25-May-21 |
| NCR Informative Emails | Kwilson,hogan |
| NCR Dispositioners | lalitha,king |
| D3 Emails | lalitha,king,fischer |
| Approval Names | Seetha-Lakshmi Lalitha | Larry King | John Fischer | John Hogan |
| Approval Signatures |  |  |  |  |
| Approval Dates |  |  |  |  |
| Approval Title | Author, SOTR | Reviewer | Reviewer | Project Manager |

|  |  |
| --- | --- |
| References | List and Hyperlink all documents related to this traveler. This includes, but is not limited to: safety (THAs, SOPs, etc), drawings, procedures, and facility related documents. |
|  | [F10040841-Rev G.pdf](file:///X%3A%5CFacilities%5CSRF%20Institute%5C01%20-%20SRF%20Projects%5C01%20-%20Open%5C1.21.01.XXX%20LCLS-II%20HE%20Project%20-%20High%20Energy%20%28Preble%5EHogan%29%5C05%20-%20Preliminary%20Drawings%20%28L2HE%29%5CF10040841Rev%20G.pdf.pdf) | [F10041603-Rev D.pdf](file:///X%3A%5CFacilities%5CSRF%20Institute%5C01%20-%20SRF%20Projects%5C01%20-%20Open%5C1.21.01.XXX%20LCLS-II%20HE%20Project%20-%20High%20Energy%20%28Preble%5EHogan%29%5C05%20-%20Preliminary%20Drawings%20%28L2HE%29%5CF10041603Rev%20D.pdf.pdf) |  |  |
|  |  |  |  |  |

|  |  |
| --- | --- |
| Revision Note |  |
| R1 | Initial release of this Traveler. |

|  |
| --- |
| **Notes**1. *The 2 K clamp assembly drawing- F10040841-Rev G.pdf.*
2. *Wear nitrile gloves while handling the components.*
 |
|  |  |
| **Figure 1: Front view of the 2 K Clamp Assembly (3D CAD model number:F10040841).**  |

|  |  |  |
| --- | --- | --- |
| **Step No.** | **Instructions** | **Data Input** |
|  | *Note: See Figure 1 and Table 1 of this document and attached CAD drawings for the details.* |
|  | **Serialization of the 2 K clamp assembly** |  |
|  | * 1. Preparer name.
 | [[Ser\_Preparer\_Name\_SRF]] <<SRF>> |
|  | * 1. Assign serial number for 2 K clamp assembly.

*Note: The labeling format is F10040841GSN where the last two digits indicate the serial number starting from 01.* | [[CLMP02KSN]] <<CLMP02KSN>> |
|  | * 1. Mark the serial number on the outer side of the 2K clamping plate (label 5 in figure 1) and 2K strap clamping plate (label 7 in figure 1)
 | [[Mark\_CLMP02KSN]] <<YESNO>> |
|  | * 1. Add comments, if any
 | [[Ser\_Comment]] <<COMMENT>> |
|  | * 1. Date of completion.
 | [[Ser\_Comp\_Date]] <<TIMESTAMP>> |
|  | **EBOM inspection** |   |
|  | * 1. Inspector name and date.
 | [[EBOMI\_Inspector\_Name\_SRF]] <<SRF>>[[EBOMI\_Date]] <<TIMESTAMP>> |
|  | * 1. Are all components listed in the Table.1 present?
 | [[EBOMI\_Tally]] <<YESNO>>[[EBOMI\_Comment]] <<COMMENT>> |
|  | * 1. If the answer is NO to step #2.2, then generate NCR.
 |  |
|  | * 1. Date of completion of EBOM inspection.
 | [[EBOMI\_Comp\_Date]] <<TIMESTAMP>> |
|  | **Visual inspection** |  |
|  | * 1. Inspector name and date.
 | [[VI\_Inspector\_Name\_SRF]] <<SRF>>[[VI\_Date]] <<TIMESTAMP>> |
|  | * 1. Are all components free of dirt, grease, oil, or chip?
 | [[VI\_Pass\_1]] <<YESNO>>[[VI\_Pass\_1\_Comment]] <<COMMENT>> |
|  | * 1. Are all parts free of sharp edges, corners, and burrs?
 | [[VI\_Pass\_2]] <<YESNO>>[[VI\_Pass\_2\_Comment]] <<COMMENT>> |
|  | * 1. Check for the signs of damage on weldments. Refer to the drawings for the 2 K clamp strip weldment (drawing no: F10041603-Rev D) for details.
 | [[VI\_Pass\_3]] <<YESNO>>[[VI\_Pass\_3\_Comment]] <<COMMENT>> |
|  | * 1. If the answer is NO to steps #3.2 and/or #3.3 and/or #3.4, then generate NCR.
 |  |
|  | * 1. Date of completion of visual inspection.
 | [[VI\_Comp\_Date]] <<TIMESTAMP>> |
|  | Re-pack the 2 K clamp assembly kit. Send to inventory area until use. | [[Repack\_Inspector\_Name\_SRF]] <<SRF>>[[Repack\_Comp\_Date]] <<TIMESTAMP>> |
|  |  |  |