|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Traveler Title | Field Probe Port Fabrication Traveler | | | |
| Traveler Abstract | Outlines the inspection and fabrication steps for the Field Probe Port Assembly for the EIC 197MHz Crab Cavity after returning from ultrasonic inspection. | | | |
| Traveler ID | EIC197-FAB-FPP-ASSYF | | | |
| Traveler Revision | R1 | | | |
| Traveler Author | J. COX | | | |
| Traveler Date | 9-Jul-24 | | | |
| NCR Informative Emails | AREILLY,GEORGED,GROSE,KDAVIS | | | |
| NCR Dispositioners | BLUMER,BUTTLES,HUQUE | | | |
| D3 Emails | AREILLY,GEORGED,GROSE,KDAVIS,BLUMER,BUTTLES,HUQUE | | | |
| Approval Names | J. COX | G. GROSE | J. BUTTLES | N. HUQUE |
| Approval Signatures |  |  |  |  |
| Approval Dates |  |  |  |  |
| Approval Title | Author | Reviewer | Project Manager |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| References | List and Hyperlink all documents related to this traveler. This includes, but is not limited to: safety (THAs, SOPs, etc), drawings, procedures, and facility related documents. | | | |
| [JL0119121](https://misportal.jlab.org/jlabDocs/documents/175657/download) | [JL0150085](https://misportal.jlab.org/jlabDocs/documents/185430/download) | [JL0139908](https://misportal.jlab.org/jlabDocs/documents/175651/download) | [JL0140270](https://misportal.jlab.org/jlabDocs/documents/175650/download) | [11141-S-0033](https://misportal.jlab.org/jlabDocs/documents/70285/download) |
| [FieldProbePortFabricationPlan](https://jeffersonlab.sharepoint.com/:p:/r/sites/EICPartnerProject-TJNAF/Accelerator/RF%20Systems/Cryomodules/197%20MHz%20DVC/Cavity%20Fabrication%20Files/Fabrication%20Plans/Field%20Probe%20Port%20Fabrication%20Plan.pptx?d=wedf4dd387d8e4bb3a8cca928b31fb420&csf=1&web=1&e=LkQEgk) This is in sharepoint, move to DS | [EIC-BPS-JL0140270](https://misportal.jlab.org/jlabDocs/documents/201698/download) | [JL0119121-Step1InspectDim](https://jeffersonlab.sharepoint.com/:b:/r/sites/EICPartnerProject-TJNAF/Accelerator/RF%20Systems/Cryomodules/197%20MHz%20DVC/Cavity%20Fabrication%20Files/Images/Traveler%20Inspection%20Dimensions/JL0119121-Step1InspectDim.pdf?csf=1&web=1&e=D8HvjT) This is in sharepoint, move to DS, it is a drawing? | [JL0150085-Step1InspectDim](https://jeffersonlab.sharepoint.com/:b:/r/sites/EICPartnerProject-TJNAF/Accelerator/RF%20Systems/Cryomodules/197%20MHz%20DVC/Cavity%20Fabrication%20Files/Images/Traveler%20Inspection%20Dimensions/JL0150085-Step1InspectDim.pdf?csf=1&web=1&e=8jOnuQ) This is in sharepoint, move to DS, it is a drawing? | [JL0139908-Step1InspectDim](https://jeffersonlab.sharepoint.com/:b:/r/sites/EICPartnerProject-TJNAF/Accelerator/RF%20Systems/Cryomodules/197%20MHz%20DVC/Cavity%20Fabrication%20Files/Images/Traveler%20Inspection%20Dimensions/JL0139908-Step1InspectDim.pdf?csf=1&web=1&e=6LUYpn) This is in sharepoint, move to DS, it is a drawing? |
| [JL0140270-Step5InspectDim](https://jeffersonlab.sharepoint.com/:b:/r/sites/EICPartnerProject-TJNAF/Accelerator/RF%20Systems/Cryomodules/197%20MHz%20DVC/Cavity%20Fabrication%20Files/Images/Traveler%20Inspection%20Dimensions/JL0140270-Step5InspectDim.pdf?csf=1&web=1&e=DUlKDC) This is in sharepoint, move to DS, it is a drawing? | [JL0140270-Step11InspectDim](https://jeffersonlab.sharepoint.com/:b:/r/sites/EICPartnerProject-TJNAF/Accelerator/RF%20Systems/Cryomodules/197%20MHz%20DVC/Cavity%20Fabrication%20Files/Images/Traveler%20Inspection%20Dimensions/JL0140270-Step11InspectDim.pdf?csf=1&web=1&e=HMC8E2) This is in sharepoint, move to DS, it is a drawing? |  |  |  |

|  |  |
| --- | --- |
| Revision Note |  |
| R1 | Initial release of this Traveler. |

|  |  |  |
| --- | --- | --- |
| Step No. | Instructions | Data Input |
| PART IDENTIFICATION | | |
| 0 | Enter Serial Number of Finished Part (WHO STARTS THIS TRAVELER?)   |  |  |  | | --- | --- | --- | | **STEPS** | **WORK CENTER AREAS** | **ACTIONS** | | 1 | MACHSHOP | Machine to final dimensions | | 2 | CMA | Leak Check | | 3 | INSP | Final dimenionsal checks | | 4 | INV | Engrave and return to INV | | [[FPCPSN]] <<SN>>  [[FPCPNote]]{{FPCP is a new component name: FPC Port Assembly}} <<NOTE>> |

|  |  |  |
| --- | --- | --- |
| **Step No** | **Instructions** | **Data Inputs** |
| MACHINING | | |
| 1 | Machine knife edge and final dimensions.  Include job number. | [[MachTech2]] <<SRF>>  [[MachTime2]] <<TIMESTAMP>>  [[MachJobNumber2]] <<INTEGER>>  [[MachComm2]] <<COMMENT>> |

|  |  |  |
| --- | --- | --- |
| Step No. | Instructions | Data Input |
| LEAK CHECK | | |
| 2 | Leak check the assembly in accordance with 11141-S-0033  [11141-S-0033](https://misportal.jlab.org/jlabDocs/documents/70285/download) Vendor Standard Helium Leak Check Procedure  Use a copper gasket to validate compliance  Upload any relevant images/comments | [[VacTech2]] <<SRF>>  [[VacTime2]] <<TIMESTAMP>>  [[VacPass2]] <<YESNO>>  [[VacComm2]] <<COMMENT>>  [[VacFile2]] <<FILEUPLOAD>> |

|  |  |  |
| --- | --- | --- |
| **Step No** | **Instructions** | **Data Inputs** |
| **DIMENSIONAL INSPECTION** | | |
| 3 | **Verify dimensions in red on JL0140270** [JL0140270](https://misportal.jlab.org/jlabDocs/documents/175650/download)  **Take knife edge profile on FormTracer**  **Upload inspection report**  **See** [JL0140270-Step11InspectDim](https://jeffersonlab.sharepoint.com/:b:/r/sites/EICPartnerProject-TJNAF/Accelerator/RF%20Systems/Cryomodules/197%20MHz%20DVC/Cavity%20Fabrication%20Files/Images/Traveler%20Inspection%20Dimensions/JL0140270-Step11InspectDim.pdf?csf=1&web=1&e=HMC8E2) | [[InsTech5]] <<SRF>>  [[InsTime5]] <<TIMESTAMP>>  [[InsPass]] <<YESNO>>  [[InsComm5]] <<COMMENT>>  [[InsFile5]] <<FILEUPLOAD>> |

|  |  |  |  |
| --- | --- | --- | --- |
| Step No. | | Instructions | Data Input |
| LOGISTICS | | | |
| 4 | **Engrave serial number onto flange (WHO ENGRAVES?)**  **Upload pictures of finished assembly** | | [[FPPASN3]] <<SN>>  [[LogTime]] <<TIMESTAMP>>  [[LogFile]] <<FILEUPLOAD>> |
| 5 | **Inventory assembly (DOES THIS PART RETURN TO INVENTORY TO BE STORED?)** | | [[LogTech]] <<SRF>>  [[LogComm]] <<COMMENT>> |